

FILT&SWAP Inline filter
Active charcoal and 0.2µm microfiltration


Reference: AT50670


Specification description

FILT&SWAP duo inline anti-Legionella filter: active charcoal and 0.2µm microfiltration.

Active charcoal: reduces taste, smells and chlorine in water.

Microfiltration: retains all bacteria and other particles larger than 0.2 µm.

Filter cartridge can be replaced without changing the filter body.

Membrane surface area: 0.5m².

Capacity: 4,755 Gallons (18,000L).

Maximum lifespan: 6 months.

Filtration flow rate: 2.37 gpm (9 lpm) with integrated flow restrictor; 3.7 gpm (14 lpm) without flow restrictor at 45 psi (3 bar).

Materials: Polypropylene body. ABS plastic parts of the filter cartridge. Polyethylene microfiltration cartridge.

Temperature: 39 - 100°F (4 - 38°C).

Operating pressure: 7 - 145 psi (0.5 - 10 bar).

Connection: 3/8" compression or NPT.

Compatible with and resistant to chemical shocks (active chlorine levels up to 100 ppm for 1 hour (cumulative total) and thermal shocks (158°F / 70°C for 30 minutes).
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