

HYGIENE+ spout end
F 55/64 - 27
50 units

Reference: AT923022.50P


Specification description

HYGIENE+ free flow spout end F 55/64 - 27 for basin faucets.

With no grid or partitions in contact with the water.

Water cannot stagnate in the internal part, reducing bacterial development.

Made from Hostaform® which reduces the build-up of scale.

Chrome-plated brass collar.

Supplied in packs of 50.

Sold individually.

Can only be installed on a faucet with a restricted flow rate to ensure a good flow with no splashing.
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