**Shower head retaining collar**

For shower grab bars Ø 1-1⅓"

Reference: **AT830**

Specification description

Shower hose retaining collar for shower riser rails Ø 1 to 1⅓".

In addition to the shower head holder, fixes to the shower hose.

Retaining device: prevents shower head from coming into direct contact with the floor or the floor trap (source of bacterial contamination).